**Documentation- UTMToLatLong Application**

Instructions to use the Application:

1. Open Command Prompt as Administrator (right-click run as administrator) (Only for Windows Machines).
2. Run the following command “pyinstaller.exe --onefile --windowed filepath” (for example: pyinstaller.exe --onefile --windowed C:\Users\hp\PycharmProjects\SkylarkDrones\UTMToLatLong.py).
3. Please wait till the process completes then open the application from the location that will be specified on the last line of the process.
4. Double click the icon to open the application.
5. Choose the ‘Enter Zone No’ to enter the zone number (between 1 and 60) and click ‘OK’ to save.
6. Choose the ‘Enter Zone Letter’ to enter the zone letter (between C and X) and click ‘OK’ to save.
7. Click ‘CSV Upload’ button which prompts to choose the file location of the .csv file you wish to upload after which click ‘Select Folder’.
8. Click ‘Convert and Save’ button which converts and save new file in the location where the file with UTM coordinates are present.
9. The ‘Quit’ or ‘X’ button can be used to close the application.

**NOTE:** The Application will be generated to the location where the command prompt location is pointing to at the time of command execution.